8x8 Font Editor – Note: H19 stores font in 16 byte blocks, using 10 bytes

<https://www.min.at/prinz/o/software/pixelfont/>

|  |  |
| --- | --- |
| CRT | 12" diagonal. |
| Display Format | 25 lines of 80 characters. |
| Display Size | 6.5" high X 8.5" wide. |
| Character Size | 0.2" high X 0.1" wide (approximate). |
| Character Set | 128 characters (95 ASCII and 33 graphic). |
| Character Type | 5 x 7 dot matrix (upper case), 5 x 9 dot matrix (lower case with descenders). |
| Keyboard | 84 keys (60 alphanumeric, 12 function/control) plus a 12-key numeric pad. |
| Cursor | Blinking nondestructive underline or block (DIP switch selectable), or disabled (software selectable). |
| Cursor Controls | Up, down, left, right, home, CR, LF, back space, and tab. |
| Cursor Addressing | Relative and Direct. |
| Tab | Standard 8-column tab. |
| Refresh Rate | 60 Hz at 60 Hz line frequency.  50 Hz at 50 Hz line frequency. |
| Edit Functions | Insert and delete character or line. |
| Erase Functions | Erase page, erase to end of line, erase to end of page, erase to beginning of line, erase to beginning of page, and erase line. |
| Scroll | Auto or line/page freeze. |
| Bell | Audible alarm on receipt of ASCII BEL. |
| Video | Normal and reverse, by character. |
| Interface | EIA RS-232C at 110 to 9600 baud. |
| Communications Mode | Full or half duplex. |
| Parity | Even, odd, stick, or none. |
| Operating Temperature | 0-40°C ambient. |
| Power Requirements | 120 VAC (105-135 VAC), 50/60Hz, 37 watts.240 VAC (210-270 VAC), 50/60 Hz, 37 watts. |
| Dimensions | 13" high X 17" wide x 20" deep. |
| Weight | (33 x 43.2 x 50.8 em.)31.0 lbs. {14.1 kg) . |

. .